[data]
    Version   = "3.1"

[disks]
    1 =.,"Cirrus Logic GD542x Windows 3.1 Driver Diskette",disk1

[oemdisks]
    N =.,"Cirrus Logic GD542x Windows 3.1 Driver Diskette",vdd542x.386
	O =.\SYSTEM,"Cirrus Logic GD542x Windows 3.x Fonts Diskette",vgaoem.fo_

; !!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
: !!! The description strings should not be changed.
; !!! Changing description strings can result in old drivers not being
; !!! upgraded since Setup uses the description string to determine what
; !!! driver is installed and whether a new, upgraded driver is provided
; !!! with this version of Windows.
; !!! NOTE: Descriptions must be less then 47 characters.  Optional Work
; !!! section names count as characters, so limit descriptions to 41 chars
; !!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
;

[display]
;profile = driver,         Description of driver,                           resolution,    286 grabber,    logo code,       VDD,            386grabber,   ega.sys,   logo data,    optional work section
;
av616    = O:16_1280.drv,  "GD5426/28 v1.32B, 640x480x16",             "100,96,96",   N:vgacolor.2gr, N:vgalogo.lgo,   N:vdd542X.386,  N:avga.3gr,,             N:vgalogo.rle, a64B
av816    = O:16_1280.drv,  "GD5426/28 v1.32B, 800x600x16",             "100,96,96",   N:vgacolor.2gr, N:vgalogo.lgo,   N:vdd542X.386,  N:avga.3gr,,             N:vgalogo.rle, a84B
av1016l  = O:16_1280.drv,  "GD5426/28 v1.32B, 1024x768x16 Lrg fnt",    "100,120,120", N:vgacolor.2gr, N:vgalogo.lgo,   N:vdd542X.386,  N:avga.3gr,,             N:vgalogo.rle, a14Bl
av1016s  = O:16_1280.drv,  "GD5426/28 v1.32B, 1024x768x16 Sml fnt",    "100,96,96",   N:vgacolor.2gr, N:vgalogo.lgo,   N:vdd542X.386,  N:avga.3gr,,             N:vgalogo.rle, a14B
av216l   = O:16_1280.drv,  "GD5426/28 v1.32B, 1280x1024x16 Lrg fnt",   "100,120,120", N:vgacolor.2gr, N:vgalogo.lgo,   N:vdd542X.386,  N:avga.3gr,,             N:vgalogo.rle, a24Bl
av216s   = O:16_1280.drv,  "GD5426/28 v1.32B, 1280x1024x16 Sml fnt",   "100,96,96",   N:vgacolor.2gr, N:vgalogo.lgo,   N:vdd542X.386,  N:avga.3gr,,             N:vgalogo.rle, a24B
av1280l  = O:256_1280.drv, "GD5426/28 v1.32B,1280x1Kx256 2mb Lfnt",  "100,120,120", N:vgacolor.2gr, N:vgalogo.lgo,   N:vdd542X.386,  N:avga.3gr,,             N:vgalogo.rle, a20Bl
av1280s  = O:256_1280.drv, "GD5426/28 v1.32B,1280x1Kx256 2mb Sfnt",  "100,96,96",   N:vgacolor.2gr, N:vgalogo.lgo,   N:vdd542X.386,  N:avga.3gr,,             N:vgalogo.rle, a20B
av1256l  = O:256_1280.drv, "GD5426/28 v1.32B, 1024x768x256 Lrg fnt",   "100,120,120", N:vgacolor.2gr, N:vgalogo.lgo,   N:vdd542X.386,  N:avga.3gr,,             N:vgalogo.rle, a18Bl
av1256s  = O:256_1280.drv, "GD5426/28 v1.32B, 1024x768x256 Sml fnt",   "100,96,96",   N:vgacolor.2gr, N:vgalogo.lgo,   N:vdd542X.386,  N:avga.3gr,,             N:vgalogo.rle, a18B
av1k64l  = O:64K_1024.drv, "GD5426/28 v1.32B, 1Kx768x64K 2mb Lfnt",    "100,96,96",   N:vgacolor.2gr, N:vgalogo.lgo,   N:vdd542X.386,  N:avga.3gr,,             N:vgalogo.rle, a116Bl
av1k64s  = O:64K_1024.drv, "GD5426/28 v1.32B, 1Kx768x64K 2mb Sfnt",    "100,96,96",   N:vgacolor.2gr, N:vgalogo.lgo,   N:vdd542X.386,  N:avga.3gr,,             N:vgalogo.rle, a116Bs
av8256   = O:256_1280.drv, "GD5426/28 v1.32B, 800x600x256",            "100,96,96",   N:vgacolor.2gr, N:vgalogo.lgo,   N:vdd542X.386,  N:avga.3gr,,             N:vgalogo.rle, a88B
av6256   = O:256_1280.drv, "GD5426/28 v1.32B, 640x480x256",            "100,96,96",   N:vgacolor.2gr, N:vgalogo.lgo,   N:vdd542X.386,  N:avga.3gr,,             N:vgalogo.rle, a68B
av864    = O:64K_1024.drv, "GD5426/28 v1.32B, 800x600x64K colors",     "100,96,96",   N:vgacolor.2gr, N:vgalogo.lgo,   N:vdd542X.386,  N:avga.3gr,,             N:vgalogo.rle, a816B
av664    = O:64K_1024.drv, "GD5426/28 v1.32B, 640x480x64K colors",     "100,96,96",   N:vgacolor.2gr, N:vgalogo.lgo,   N:vdd542X.386,  N:avga.3gr,,             N:vgalogo.rle, a616B
av616M   = O:16M_640.drv,  "GD5426/28 v1.32B, 640x480x16.8M Color",    "100,96,96",  N:vgacolor.2gr, N:vgalogo.lgo,   N:vdd542X.386,  N:avga.3gr,,             N:vgalogo.rle, a624B

;
; Optional sections listed in field 9 of the display secton are interpreted as follows:
;
; File, Destination, .ini file, Section, LHS, RHS
;
; Where:    x:File      = Optional; file to be copied, may be left null.
;           Destination = 0: for windows root or 0:system for \system subdir.
;           .ini file   = Optional; .ini file to be modified or created.
;           Section     = Section of .ini file to be modified.
;           OldLine     = Optional; old line to be removed from the .ini file.
;                          Only one occurence of the specified string is removed.
;           NewLine     = New text line to be written to the .ini file.
;
[a14Bl]
,,system.ini,CLVGA,"dpi=","dpi=120"
,,system.ini,CLVGA,"videomode=","videomode=93"

[a14B]
,,system.ini,CLVGA,"dpi=","dpi=96"
,,system.ini,CLVGA,"videomode=","videomode=93"

[a24Bl]
,,system.ini,CLVGA,"dpi=","dpi=120"
,,system.ini,CLVGA,"videomode=","videomode=108"

[a24B]
,,system.ini,CLVGA,"dpi=","dpi=96"
,,system.ini,CLVGA,"videomode=","videomode=108"

[a84B]
,,system.ini,CLVGA,"dpi=","dpi=96"
,,system.ini,CLVGA,"videomode=","videomode=88"

[a64B]
,,system.ini,CLVGA,"dpi=","dpi=96"
,,system.ini,CLVGA,"videomode=","videomode=18"

[a20Bl]
,,system.ini,CLVGA,"dpi=","dpi=120"
,,system.ini,CLVGA,"videomode=","videomode=109"

[a20B]
,,system.ini,CLVGA,"dpi=","dpi=96"
,,system.ini,CLVGA,"videomode=","videomode=109"

[a18Bl]
,,system.ini,CLVGA,"dpi=","dpi=120"
,,system.ini,CLVGA,"videomode=","videomode=96"

[a18B]
,,system.ini,CLVGA,"dpi=","dpi=96"
,,system.ini,CLVGA,"videomode=","videomode=96"

[a88B]
,,system.ini,CLVGA,"dpi=","dpi=96"
,,system.ini,CLVGA,"videomode=","videomode=92"

[a68B]
,,system.ini,CLVGA,"dpi=","dpi=96"
,,system.ini,CLVGA,"videomode=","videomode=95"

[a116Bs]
,,system.ini,CLVGA,"dpi=","dpi=96"
,,system.ini,CLVGA,"videomode=","videomode=116"

[a116Bl]
,,system.ini,CLVGA,"dpi=","dpi=120"
,,system.ini,CLVGA,"videomode=","videomode=116"

[a816B]
,,system.ini,CLVGA,"dpi=","dpi=96"
,,system.ini,CLVGA,"videomode=","videomode=101"

[a616B]
,,system.ini,CLVGA,"dpi=","dpi=96"
,,system.ini,CLVGA,"videomode=","videomode=100"

[a624B]
,,system.ini,CLVGA,"dpi=","dpi=96"
,,system.ini,CLVGA,"videomode=","videomode=113"

[avga.3gr]
O:CGA40WOA.FON,O:CGA40850.FON
O:CGA80WOA.FON,O:CGA80850.FON
O:EGA40WOA.FON,O:EGA40850.FON
O:EGA80WOA.FON,O:EGA80850.FON

[sysfonts]
O:vgasys.fon,"VGA (640x480) resolution System Font", "100,96,96"
O:8514sys.fon,"Super VGA (1024x768) resolution System Font", "100,120,120"

[fixedfonts]
O:vgafix.fon,"VGA (640x480) resolution Fixed System Font", "100,96,96"
O:8514fix.fon,"Super VGA (1024x768) resolution Fixed System Font",  "100,120,120"

[oemfonts]
O:vgaoem.fon,"VGA (640x480) resolution Terminal Font (USA/Europe)", "100,96,96",1
O:8514oem.fon,"Super VGA (1024x768) resolution Terminal Font (USA/Europe)", "100,120,120",1

[fonts]
   O:SSERIFE.FON, "MS Sans Serif 8,10,12,14,18,24 (VGA res)", "100,96,96"
   O:SSERIFF.FON, "MS Sans Serif 8,10,12,14,18,24 (Super VGA res)", "100,120,120"

   O:COURE.FON, "Courier 10,12,15 (VGA res)", "100,96,96"
   O:COURF.FON, "Courier 10,12,15 (Super VGA res)", "100,120,120"

   O:SERIFE.FON, "MS Serif 8,10,12,14,18,24 (VGA res)", "100,96,96"
   O:SERIFF.FON, "MS Serif 8,10,12,14,18,24 (Super VGA res)", "100,120,120"

   O:SYMBOLE.FON, "Symbol 8,10,12,14,18,24 (VGA res)", "100,96,96"
   O:SYMBOLF.FON, "Symbol 8,10,12,14,18,24 (Super VGA res)", "100,120,120"

   O:SMALLE.FON, "Small Fonts (VGA res)", "100,96,96"
   O:SMALLF.FON, "Small Fonts (Super VGA res)", "100,120,120"

   O:ROMAN.FON, "Roman (Plotter)",   "CONTINUOUSSCALING"
   O:SCRIPT.FON, "Script (Plotter)", "CONTINUOUSSCALING"
   O:MODERN.FON, "Modern (Plotter)", "CONTINUOUSSCALING"
